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NOTES:

[F THE ACTUATOR IS ORDERED WITHOUT A VALVE,
PERFORM THE FOLLOWING OPERATIONS BEFORE
LABELING AND PACKAGING FOR SHIPMENT:

1. EXTEND THE ACTUATOR UNTIL IT SHUTS OFF, THEN
REMOVE ACTUATOR FROM THE TEST VALVE.

@ 2. SLIDE ITEM 37A INTO THE ACTUATOR SO THAT IT IS
LOADED AGAINST THE BOTTOM SURFACE OF THE
DRIVE SCREW (THIS WILL KEEP THE DRIVE SCREW
FROM ROTATING). THEN, TIGHTEN ITEM 35
(INDICATOR NUT).

@ 3. HIGHPOT THE ACTUATOR AT 1500 VOLTS FOR 1 SEC.
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FRAC-218-1 GEAR PIN THREE (MID-LENGTH)
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24 [BRF-3251-10 OF 23
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56 1BCS.51-194 MOBILE RED GREASE RI®)
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| 35 [FRAC-219-18  |INDICATOR NUT
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| 37 [FRAC-251-18 [STEM EXTENSION (BRASS WITH HEX) (D3)ES) PACKAGING PREP
I I () T ASSEMBLY
3. ] | 1@ (1/2 SCALE)
| 39 [H6-18  |INSTANT ADHESIVE

| 40 |E-22-93-030 ()  [sooeR 0000000000000 |e/Rje/R]
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PACKAGING

BOX P/N: BOX-1882
INSERT P/N: BOX-1@83
G.I. SHEET: F-26264

LABEL: PART NO., DESCRIPTION,
(LBL-ZEBRA-2)| DATE CODE AND "CE* MARK
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POSITION (CABLE) ITEM 22
AS SHOWN, WITH (WIRE TIE)
ITEM 23 INSIDE (BASE) ITEM 1
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(1B) MACHINE PER FRAC-247-XXX-1 DRAWING.
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PRESS ITEMS 2, 3,
& 4 INTOITEM 1 TO
HEIGHT SPECIFIED.
PIN 2 MUST BE
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SEC A-A

ITEMS 1A & 28 (SHOWN)
ORITEM 1B

PRESS ITEM 18 ONTQ
ITEM 11, ITEM 18 TO
BE FLUSH WITH END OF
MOTOR SHAFT +/-.028.
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() or (%)

INSTALLATION
TORQUE: 35-45
IN-LBS

REMOVE INSULATION
ON ALL WIRES .125/
508 THIS END ONLY.

REMOVE JACKET
4.000" +/-.250"

MACHINE PER
FRAC-248-1 DRG
SPECIFICATIONS

SOLDERED WIRES CANNOT
EXTEND MORE THAN .293"
BEYOND BACK OF BOARD
SURFACE.

1. DRIVE IN MOTOR SCREWS
(ITEM 5) HALF WAY.

2. ROTATE MOTOR EITHER
DIRECTION UNTIL MOTOR
SCREW SLOTS STOP
AGAINST SCREWS.

3. TORGUE SCREWS TO

8-10 IN.-LBS.

COM - BLK
EXT - RED

RET - WHITE @
GND - GREEN

SOLDER WIRES INTO P.C.B.
(B) USING ITEM 4@.

SEE CABLE
ASS’Y.

NOTE:
SMALL DIA.
END UP.

THREAD ITEM 14 INTO ITEM 15

TO APPROX. .375 BELOW TOP
SURFACE OF ITEM 15. @@

ADD (APPROX. .04 GRAMS) OF ITEM 26 TO THE
THREADS (TO KEEP DRIVE SCREW IN POSITION).
POSITION SO THAT THE DISTANCE FROM THE
BOTTOM OF THE ACTUATOR TO THE BOTTOM OF
DRIVE SCREW IS 1.809 +/-.015,

NOTE: KEEP INSIDE OF ACTUATOR FREE
OF ITEM 26.

MACHINE PER
FRAC-247-XXX-1
DRWG. SPEC’S.

TORQUE TO
8-10 IN/LBS.

@

PLACE A BEAD OF ITEM 33 (APPROX. .0908 DIA.)

ITEM 21 FROM AROUND THE INTERFACE BETWEEN THE THIRD
CABLE ASSEMBLY. SPRING AND ITEM 38@.
(.030
THICK)
' l 77 (.030
TORQUE TO .__... THICK
l// (.03 @
THICK) TYP (4)
(.30 -
THICK) P
ASSY. 'A’ ASSY. "'B"

STACK ITEM #13 SPRINGS WITH BEVELED
SIDES IN POSITION SHOWN.
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REMOVE JACK
2.125" +/-.125"

CABLE ASSEMBLY
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WITH ITEM 32 ATTACHED AS
SHOWN IN RELATION TO ITEM
15, ASSEMBLY PCB (ITEM 16)
ALONG WITH GEAR (ITEM 15)
INTO BASE (ITEM 1.
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SCHEMATIC

TIGHTEN WIRE TIE SO THAT
WIRE TIE WILL NOT SLIP
WITH A 20 LB. (REF. LOAD)
APPLIED TO THE CABLE.

REMOVE INSULATION ON
ALL WIRES .218/.125
AND SOLDER TO PCB AS
PER COLOR CODE BELOW.

CRIMP ITEM 21 TO
THIS END OF GREEN
WIRE.

TO ATTACH SWITCH ACTUATOR
(ITEM 32) TO THE PCB (ITEM 16):
PUSH THE HOOK ON ITEM 32 INTO
;gg RECTANGULAR HOLE IN THE

NOTE: INSURE ITEM iiF iS FULLY

SEATED AT SURFACE[-A-] OF PCB.
(B) THEN, APPLY A DROP OF 1TEM 39
BETWEEN ITEMS 16 AND 32.
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