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What’s fixed in “PL7 V4.5 Service Pack1”

This patch is available on the website, www.telemecanique.com (Library/Resolutions). 

This document describes the content of quality problems and improvement provided by the Service Pack1 for the PL7 V4.5 version.

Included in the V4.5/SP1 Patch

This service pack contains the following warnings and updates:

1. Registration and Transfer of User Rights

2. OLE Functions

3. Exporting protected DFBs

4. TSXMFPP001M Memory Card

5. Module TSX PBY 100 with a German version of PL7

6. Connection to an PLC with a version of PL7 Italian or Spanish

7. Uninstalling a version of PL7

1 - Registration and Transfer of User Rights

· Automatic registration of PL7 V4.5 from an authorized version V4.4

· Registering PL7 V4.5 on a workstation with an operating system installed on a hard drive other than C:\

· Registering PL7 V4.5 on a workstation with a dual boot system

· Transfer of Network User Rights: 
When performing an Authorization Transfer on a network, the folder ..\PL7\PL7PRO45\EXE on the target workstation must be a shared folder.

2- OLE Automation Server Functions

· "DownloadStationWithSymbol" execution error:
Integrate DownloadStationWithSymbol (String p_IpDriver, String p_IpAdresse). This function allows you to load an application and its compressed database in the PLC.

· "CompareSymbolPCAndSymbolPLCAppli" execution error: 
Integrate CompareSymbolPCAndSymbolPLCAppli (VARIANT FAR* p_pVarInfo i). This function may be used to obtain general information about an application contained in a PLC.

*Reminder: Only the PL7 V4.5 VisualC++ sample integrates the use of these 2 new functions.

3- Exporting protected DFBs 

· Improved export of PL7 FEF files, for password-protected DFBs.

· Export of protected DFBs is dedicated to the UnityPro PL7Conveter
The SP1 adds an ExportPl7Converter keyword in the PL7SYS.INI file.

 * FALSE (default value): the export is unchanged, all external tools using the FEF format are still compatible
* TRUE: export of protected DFBs is generated in the FEF file for conversion in Unity Pro (see the following documentation: conversion of applications in Unity Pro) 

4 - TSXMFPP001M Memory Card

· Support for the new Flash EPROM memory extension application: TSXMFPP001M PV05
It offers a program capacity of 256 Kwords (512 KB). It is configurable in all Premium and Atrium processors of level 57-20, 30 and 40 starting from version V5.5.

5 - Module TSX PBY 100 with a German version of PL7

· Configuration of the module Profibus TSX PBY 100 with PL7 V4.5 installed in German language.

6 - Connection to an PLC with a version of PL7 Italian or Spanish

· Reconnexion with a PLC following a modification of the application with PL7 V4.5 installed in Italian or Spanish.

7 - Uninstalling a version of PL7

· If several versions of PL7 are installed in the same workstation, during uninstall it is recommended to select only the kernel and keep the common components

