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The access switch on the remote keypad display is used as follows:

Locked Position £: Only monitoring parameters can be accessed. When
the starter is running, it is not possible to select a different parameter to
be displayed.

Partial Locked Position O: Limited access to the SEt, PrO, and SUP
menu parameters.

Unlocked Position =': All parameters are accessible.
Any display restrictions to the starter by the access switch will still be in

force once the remote keypad display has been disconnected from the
controller, even if power to the controller is cycled.




