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Table D.8 — Faults and fault exclusions — Switches — Electromechanical position switches,
‘manually operated switches (e.g. push-button, reset actuator, DIP switch,

magnetically operated contacts, reed switch, pressure s

h, temperature switch)

Fault considered

Fault exclusion

Contact will not close

Pressure-sensitive devices in accord-
ance with ISO 13856

Contact will not open

Contacts in accordance with
1EC 60947-5-1:2003, Annex K, are
expected to open.

For PL e, a fault exclusion for mechanical (e.g. the mechanical link between an actuator and a contact element)
and electrical aspects s not allowed. In this case redundancy is necessary. For emergency stop devices in
accordance with IEC 60947-5-5, a fault exclusion for mechanical aspects is allowed if a maximum number of

operations is considered.

NOTE  The faultlists for the mechanical aspects are considered in Annex A.





