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Both the RM22JA31MR and RM22JA31MR SP01 product having similar specification except the function diagram.

RM22JA31MR	, Function diagram >>> Positive Logic.
RM22JA31MRSP01, Function diagram >>> Negative logic.
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Notes:
The behaviour of the output relay signal is different.  
Please refer to the instruction sheet for more detail information.
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