## Import an SCL

1. Right-click on the desired substation, voltage level or bay and select Import SCLSubstation Configuration Language.
2. Select the .SCDSubstation Configuration Description file to open and click OK.
3. In the main document window a new tab named "Import: Path to selected file"appears.
4. To view the SCL source click the View SCL button.
5. To import a device, enable the relevant checkbox and click Import to[...]. More than one device may be selected.