## Extract Overload Recordings

The Extract Overload download functions are provided only for Px30-related products. They are not supported for Px40, Px20 or Px10/V11x models.

### Extract an Overload Recording

1. Right-click on the Log Records of a Px30 device in Studio Explorer and select Extract Overload Records.
2. The resulting Extracting Log Records from Devicegeneric name for any piece of equipment that can be communicated with using Courier. dialog will show the progress of the extraction.
   The filename will start with the type of file which is being extracted, namely:
   OPROperating Data Records is Operating Data Records
   MNRMonitoring Data Records is Monitoring Data Records
   OLROverload Records is Overload Records
   The filename will also include the date and time the extraction was made. An example filename might be:
   OLR 2012-03-19 15.47.50
3. After successful extraction, a list of overload recordings is shown in the Overload Recordings selection window.
4. Select the recording you have just made, and you can type some explanatory text in the User Comment dialog box. Click the OK button to return to the Overload Recordings selection window.

### View an Overload Recording

Either:

- Double-click on the required Log Record of a Px30 device in Studio Explorer OR
- Right-click on the required Log Record of a Px30 device in Studio Explorer and select Open File.