## MiCOM S1 Studio Menus

The MiCOM S1 Studio software has a menu bar and several other right-click menus. A list of these is given below.

- Menu Bar
- Studio Explorer Toolbar
- Studio Explorer Right-Click Menus
- Document Toolbar
- Document Right-Click Menus

### Menu Bar

The MiCOM S1 Studio software has these menus.

- Quick Connect
- Px10 Series
- Front USB Port
- Rear Serial Port
- Px20 Series
- Front port
- Modbus rear port
- CourierThe communications language developed to provide generic control, monitoring, data extraction and setting changes on remote devices within the substation environment. rear port
- Px30 Series
- Serial port
- Ethernet port
- File transfer mode via Serial port
- Px40 Series
- Front port
- Rear port
- Ethernet port
- P741/P732/P732
- Front port
- Rear port
- Ethernet port
- Modulex Series
- K Series
- L Series
- M720
- File
- Open Default File
- Settings FileThe complete set of settings for a device. This may include one or more alternative Settings Groups....
- DNP3 File (Px40)...
- PSL File (Px40)...
- MCL 61850 File...
- BTC FIle (Px30)...
- UCA2 GOOSE File (Px40)...
- Devicegeneric name for any piece of equipment that can be communicated with using Courier. Text File (Px40)...
- Open File
- Px10/Px20/Px20C/M/Modulex
- Settings File...
- Events File...
- Disturbance Recorddata record of a disturbance on the power system that has been recorded by a device. File...
- Px30/Px30C/Cx30/PG88/PH89
- Settings File...
- MCL 61850 FIle...
- Bay Template Configurator File...
- Log Record File...
- Disturbance Record File...
- Px40/K/L/Px20(Courier)
- Settings File...
- DNP3 Settings File...
- PSL File...
- MCL 61850 File...
- UCA2 GOOSE File...
- Device Text File...
- Events File...
- Disturbance Record File...
- New System
- Open System
- Delete System
- Close System
- Compact System
- Export System
- Import System
- Import SCLSubstation Configuration Language
- Recent Systems
- Exit
- View
- Start PageAn individual topic within a Help system.
- Search Results
- Properties
- Studio Explorer
- Print
- Print...
- Print Preview
- Page Setup...
- Tools
- IEC 61850 IEDIntelligent Electronic Device. A device that initiates the disconnection of part of an electrical installation, and / or operates a warning signal when a fault or abnormal condition occurs, with minimum disruption of service. May also be known as a Relay. Configurator
- PSL Editor (Px40)
- PSL Editor (Px30)
- BTC Editor (Px30)
- DR Viewer: WaveWin
- DR Viewer: EView
- Text Editor
- IEC61850 IED Configurator
- Device Text Editor (Px40)
- Device Text Editor (Px30)
- Options
- Language
- List of Languages
- Preferences...
- Help
- S1 Studio Help
- Contact Schneider Electric
- Register MiCOM S1 Studio
- MiCOM S1 Studio Web Page
- About...

Some of these options are shown/hidden depending on which section of the interface you are currently using. Options which are not relevant to your current task may be hidden from view.

### Studio Explorer Toolbar

The icons shown on the Explorer toolbar vary depending on which element is currently highlighted. They include:

IconA picture or symbol that represents an object, task, command, or choice users can select by pointing and clicking with a mouse. | Nothing Highlighted | System | Substation | Voltage Level | Bay | Device | Connections | ConnectionAn active link between a computer and a device through which data can be sent. | Settings | Measurements | Events | Disturbance Records | File
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
New System | Yes |  |  |  |  |  |  |  |  |  |  |  |
Open System | Yes |  |  |  |  |  |  |  |  |  |  |  |
Send |  | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
New Device |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
New Substation |  | Yes |  |  |  |  |  |  |  |  |  |  |
New Voltage Level |  |  | Yes |  |  |  |  |  |  |  |  |  |
New Bay |  |  |  | Yes |  |  |  |  |  |  |  |  |
Supervise Device |  |  |  |  |  | Yes |  |  |  |  |  |  |
New Connection... |  |  |  |  |  |  | Yes |  |  |  |  |  |
Add predefined connection |  |  |  |  |  |  | Yes |  |  |  |  |  |
Test connection |  |  |  |  |  |  |  | Yes |  |  |  |  |
New File |  |  |  |  |  |  |  |  | Yes | Yes |  |  |
Add Existing File... |  |  |  |  |  |  |  |  | Yes | Yes | Yes | Yes |
Extract Settings |  |  |  |  |  |  |  |  | Yes | Yes |  |  |
Extract Events |  |  |  |  |  |  |  |  |  |  | Yes |  |
Extract Disturbances |  |  |  |  |  |  |  |  |  |  |  | Yes |
Open |  |  |  |  |  |  |  |  |  |  |  |  | Yes
Rename |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  | Yes
Edit |  |  |  |  |  |  |  | Yes |  |  |  |  |
Close |  | Yes |  |  |  |  |  |  |  |  |  |  |
Delete |  | Yes | Yes | Yes | Yes | Yes |  | Yes |  |  |  |  | Yes
Cut |  |  | Yes | Yes | Yes | Yes |  | Yes |  |  |  |  | Yes
Copy |  |  | Yes | Yes | Yes | Yes |  | Yes |  |  |  |  | Yes
Paste |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |
Explore |  | Yes | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes | Yes |
Properties |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes
Options |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes

### Studio Explorer Right-Click Menus

These vary depending on which element of the MiCOM S1 Studio interface is currently highlighted. They include:

Menu option | System | Substation | Voltage Level | Bay | Device | Connections | Connections File | Settings | Settings File | Measurements | Measurements File | Events | Disturbance Records
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Send... | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
Extract All Records... | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
Extract All Configurations... | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
Export | Yes |  |  |  |  |  |  |  |  |  |  |  |
Compact... | Yes |  |  |  |  |  |  |  |  |  |  |  |
New Device | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |
New Substation | Yes |  |  |  |  |  |  |  |  |  |  |  |
New Voltage Level |  | Yes |  |  |  |  |  |  |  |  |  |  |
New Bay |  |  | Yes |  |  |  |  |  |  |  |  |  |
Supervise Device |  |  |  |  | Yes |  |  |  |  |  |  |  |
New Connection |  |  |  |  |  | Yes |  |  |  |  |  |  |
Add predefined connection -> |  |  |  |  |  | Yes |  |  |  |  |  |  |
-> Modbus Serial |  |  |  |  |  | Yes |  |  |  |  |  |  |
-> Modbus Px10 Front Usb |  |  |  |  |  | Yes |  |  |  |  |  |  |
-> Modbus Px10 Rear Serial |  |  |  |  |  | Yes |  |  |  |  |  |  |
-> Modbus Px20 Front |  |  |  |  |  | Yes |  |  |  |  |  |  |
-> Modbus Px20 Rear |  |  |  |  |  | Yes |  |  |  |  |  |  |
-> Modbus Modulex |  |  |  |  |  | Yes |  |  |  |  |  |  |
-> Modbus M Series |  |  |  |  |  | Yes |  |  |  |  |  |  |
Test Connection |  |  |  |  |  |  | Yes |  |  |  |  |  |
New File |  |  |  |  |  |  |  | Yes |  | Yes |  |  |
Add Existing File |  |  |  |  |  |  |  | Yes |  | Yes |  | Yes | Yes
Extract Settings |  |  |  |  |  |  |  | Yes |  |  |  |  |
Open |  |  |  |  |  |  |  |  | Yes |  | Yes |  |
Open in Other Language |  |  |  |  |  |  |  |  | Yes |  |  |  |
Export to CSV or CAPE... |  |  |  |  |  |  |  |  | Yes |  |  |  |
Convert Settings File... |  |  |  |  |  |  |  |  | Yes |  |  |  |
Compare - First File |  |  |  |  |  |  |  |  | Yes |  |  |  |
Compare with External File... |  |  |  |  |  |  |  |  | Yes |  |  |  |
Extract Events |  |  |  |  |  |  |  |  |  |  |  | Yes |
Extract Disturbances |  |  |  |  |  |  |  |  |  |  |  |  | Yes
Edit |  |  |  |  |  |  | Yes |  |  |  |  |  |
Rename | Yes | Yes | Yes | Yes | Yes |  |  |  | Yes |  | Yes |  |
Close | Yes |  |  |  |  |  |  |  |  |  |  |  |
Delete | Yes | Yes | Yes | Yes | Yes |  | Yes |  | Yes |  | Yes |  |
Cut |  | Yes | Yes | Yes | Yes |  | Yes |  | Yes |  | Yes |  |
Copy |  | Yes | Yes | Yes | Yes |  | Yes |  | Yes |  | Yes |  |
Paste | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  | Yes | Yes
Explore | Yes | Yes | Yes | Yes | Yes |  |  | Yes |  | Yes |  | Yes | Yes
Properties | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes

#### Document Toolbar

The Document Toolbar has these icons.

- View
- Only Modified Settings
- Only Editable Settings
- File comments
- Save
- Save As
- Copy

The document Toolbar also has a Search box, which allows you to search for any entries which meet your search criteria.

The view toolbar options let you view only those settings which have been modified and/or this which can actually be edited.

The File Comments icon allows you to record a description of the whole File.

The Save, Save As and Copy icons allow you to save and make copies of the file for the purposes of archive or re-use elsewhere.

#### Document Right-Click Menus

The Document Right-Click Menu has these options.

- Edit Value
- Change User Note
- Extracting Settings from Device
- Send Data to Device
- Copy Selection
- Collapse
- Collapse all
- Expand
- Expand all

Note some of these menu options will be hidden if the highlighted row can not be edited.

The Edit Value option lets you edit the value of the currently highlighted row.

The Change User Note option lets you record a comments about the currently highlighted row.

The Collapse/Expand options let you expand or collapse sections of the document.