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The external supply must follow recommendation below:
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The cable must be a shielded cable and connected to the earth like shown on STOA/STOB wiring ( on picture above)
 
[image: ]
 

Public

Public

Public

image1.png
3

Wiring diagram for frame sizes 1.
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NOTE: The +24VDC power supply must meet the requirements of I[EC 61131-2 (PELV standard power
supply unit).
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e Safe torque off inputs STOA / STOB use shielded cables and one common 24V line. This 24V line is
used only for STOA / STOB.




