Version:
========
UPS 01.2

Applicable Models:
==================
SRTL8KRM4UI
SRTL8KRM4UT
SRTL8KRM4UJ
SRTL10KRM4UI
SRTL10KRM4UT
SRTL10KRM4UJ

Compatibility:
==============	
1. NMC SUCAN v2-4-1-4 and above required to upgrade the UPS:
Note: If NMC SUCAN Version is below 2-4-1-4 version, Below Web link helps in upgrading the APC NMC Card with latest NMC SUCAN version. 
      https://www.apc.com/us/en/faqs/FA156047/
2. NMC SUCAN v2-4-1-4 will support firmware upgrade with output OFF.
3. Web Link for instructions to upgrade the UPS Firmware using NMC - https://www.apc.com/us/en/faqs/FA170679/

Release Notes (UPS 01.2):
========================
SRTL8KRM4UI, SRTL8KRM4UT, SRTL8KRM4UJ, SRTL10KRM4UI, SRTL10KRM4UT, SRTL10KRM4UJ

1. Improved algorithm to eliminate false trigger of Bypass Relay weld at no load.
2. Battery firmware version updated to v0.8.47 to resolve the false triggering of battery module End Of Life event.
3. Improved firmware upgrade functionality for XBP(External Battery Pack). 
4. Added Battery fuse open detection logic.

Release Notes (UPS 01.1):
========================
SRTL8KRM4UI, SRTL8KRM4UT, SRTL8KRM4UJ, SRTL10KRM4UI, SRTL10KRM4UT, SRTL10KRM4UJ

1. Improved algorithm to detect Power Module severe over-voltage logic.
2. Improved system handling for over-temperature conditions.
3. The text translation for Japanese language has been improved in the LCD UI.
4. Improved line-battery relay weld detection logic.
5. Increased the buffer from 20 to 30 to address the overflow of events when 10 XBPs are connected.
6. Addressed charger power toggling when 10th XBP connected.

Release Notes (UPS 01.0):
========================
SRTL8KRM4UI, SRTL8KRM4UT, SRTL8KRM4UJ, SRTL10KRM4UI, SRTL10KRM4UT, SRTL10KRM4UJ

1. Improved recovery mechanism for output voltage transient.
2. Implemented Abort functionality to stop UPS firmware upgrade using display.
3. Optimsed the algorithm to clear overload warning once the load had been reduced.
4. Addressed battery replacement date and replacement warning in display.
5. Resolved the battery module End Of Life warning by reducing the SOH from 80% to 70%. 
6. Improved system behavior to eliminate false trigger of warning related to battery module during low battery shutdown.
7. Resolved the outlets loadshed time setting mismatch between NMC and display. 
