-----------------------------------------------------------------------------------------------------------------------------------------------
Steps to add device support for ION9000 and 9810 V2.0.0 in PME 7.2.x Primary Server and Standalone Server
-----------------------------------------------------------------------------------------------------------------------------------------------

1. Extract both ION9000_V2.0.0_SharedAssets.zip and ION9000_V2.0.0_LocalAssets.zip to the installed path root, such as "C:\Program Files (x86)\Schneider Electric\ION Enterprise"
	Notes: 
	- if prompted to merge the folders, click Yes. 
	- the following files may already exist in your PME system.  You may choose to replacing the existing ones with the new ones.
		panel - full x half.bmp
		panel - half x full.bmp
		panel - half x half.bmp
		panel - half x third.bmp
		panel - links.bmp
		panel - third x full.bmp
		panel - two thirds wide x third.bmp
		panel - two thirds wide x two thirds.bmp
		panel - two thirds x half.bmp
		_9000.bmp
		_9810.bmp

2. Open Windows Command Prompt and go to the system bin folder, such as "C:\Program Files (x86)\Schneider Electric\ION Enterprise\system\bin"

3. Run the following commands in the Windows Command Prompt:
	MeterRegistry.exe Registry9810V2.0.0.xml
	MeterRegistry.exe RegistryION9000V2.0.0.xml

4. Open SQL Management Studio, connect to your database server where your PME databases are installed.

5. Open and execute the ION9000_V2.0.0.sql in the Diagnostic folder, such "C:\Program Files (x86)\Schneider Electric\ION Enterprise\Diagnostic":
	Notes:
	- If you don't have SQL Management Studio on your Primary Server, you will have to run this script on your database server where your PME databases are installed.
