## Quick Settings File Guide

Before using this functionality, please read the Extended Platform Devices topic, as this explains the differences between the two types of protocols for the extraction of data.

Default settings files opened with Open Default File + SettingThe information held within a single data location in a Courier database. File cannot be sent to a device.

To create a settings file to send to a specific device, first create a device using Quick Connect or add a device. You can then create a new settings file for the device.

Use the following method to open any default settings file installed with S1 Studio that will not be sent to a device:

1. Click on File from the menu-bar.
2. Select Open Default File + Settings FileThe complete set of settings for a device. This may include one or more alternative Settings Groups..
3. Select a device type from the Select Device TypeVariants of a device each with different specifications and features. dialog.
4. Select a relay type from the Select Type dialog and click Next.
5. Select a language and model from the Select Model dialog and click Finish.
6. The default settings file will be displayed in the main window area.

#### See also:

- Extract full settings from a device
- Extract settings from a device
- Change settings
- Send settings to a device
- Extended Platform Devices