## Bay Template Configuration (BTC)

#### To access the Bay Template Configuration (BTC) Module:

1. Expand the System in the Studio Explorer pane until you can see the bay you wish to configure.
2. Highlight the bay you wish to configure, then click the Tools + BTC Editor menu option
3. The BTC Editor module window will then be opened, allowing you to edit the Bay.
4. The MiCOM S1 Studio software will be locked whilst the BTC Editor Module window is opened. It will be unlocked once the BTC Editor Module window is closed.

Important

The BTC module supports MiCOM (Px3x and Cx3x) products only.
Details of how to use the BTC editor module are given in the on-line help for that application.