### Enable Server, Sites, and Devices

Configuration Manager leaves the server, sites, and devices in a disabled state after Write to System. This is a safety precaution to ensure that the PME system does not go into service until it is ready and its correct configuration has been verified.

warning

unintended equipment operation

Do not use the software for critical control or protection applications where human or equipment safety relies on the operation of the control action.

Do not use the software to control time-critical functions because communication delays can occur between the time a control is initiated and when that action is applied.

Do not use the software to control remote equipment without securing it with an authorized access level, and without including a status object to provide feedback about the status of the control operation.

Failure to follow these instructions can result in death or serious injury.

Perform all required manual tasks, especially installing missing device drivers, and then enable the server, sites, and devices through the Management Console.

Test that each device can display the default diagram. If communication problems exist, address them before proceeding.